The LCD pinout works with parallel interface type LCD's with or without backlight.
If for some reason your LCD Contrast is not looking right you can replace resistor at R3 to a value that works for your LCD.
If you change the power setting to 3.3V you will also need to change the resistor to get proper contrast.