The BMP085 on the breadboard is a Sparkfun breakout board click on the image for a link. Same goes for the LCD just click on the image to a link of the product page. The pyMCU board is configured to run in 3.3V power mode based on the specs required by the BMP085 chip.
